(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(comment 4 "AISLER Project ID: UDKLLJUE")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "VCC")
	(net 2 "GND")
	(net 3 "A")
	(net 4 "B")
	(net 5 "C")
	(footprint ""
		(layer "F.Cu")
		(at 236.22 68.58)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Library:pad_2Dmm_1Fmm"
		(layer "F.Cu")
		(at 236.22 53.34)
		(property "Reference" "REF**"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "pad_2Dmm_1Fmm"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 81.28)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 76.2)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 68.58)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 73.66)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 76.2)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 101.6)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 99.06)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 78.74)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 58.42)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 243.84 106.68)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 63.5)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 238.76 63.5)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 81.28)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 78.74)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 88.9)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 81.28)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 66.04)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "F.Cu")
		(at 241.59 75.08 90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "REF**"
			(at 3.25 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_PUSH_6mm"
			(at 3.75 6.7 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "B"
			(at 3.25 2.25 0)
			(unlocked yes)
			(layer "F.Cu")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "B")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "B")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 55.88)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 66.04)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 91.44)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "F.Cu")
		(at 241.59 97.94 90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "REF**"
			(at 3.25 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_PUSH_6mm"
			(at 3.75 6.7 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "A"
			(at 3.25 2.25 0)
			(unlocked yes)
			(layer "F.Cu")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "A")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "A")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 93.98)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "F.Cu")
		(at 241.59 52.22 90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "REF**"
			(at 3.25 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_PUSH_6mm"
			(at 3.75 6.7 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "C"
			(at 3.25 2.25 0)
			(unlocked yes)
			(layer "F.Cu")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "C")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "C")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 86.36)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 93.98)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 234.948451 47.79722)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 101.6)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 66.04)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 73.525163)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 63.5)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 88.9)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 63.5)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 238.76 60.96)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 86.36)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 86.36)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 60.96)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 91.44)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 83.82)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 99.06)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 60.96)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 248.92 88.9)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 233.68 53.34 180)
		(descr "Through hole straight socket strip, 1x20, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x20 2.54mm single row")
		(property "Reference" "REF**"
			(at 0 2.77 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "PinSocket_1x20_P2.54mm_Vertical"
			(at 0 -51.03 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "3" thru_hole circle
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "5" thru_hole circle
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(pad "6" thru_hole circle
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "7" thru_hole circle
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "8" thru_hole circle
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "9" thru_hole circle
			(at 0 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "10" thru_hole circle
			(at 0 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "11" thru_hole circle
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "12" thru_hole circle
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole circle
			(at 0 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "14" thru_hole circle
			(at 0 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole circle
			(at 0 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "16" thru_hole circle
			(at 0 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "17" thru_hole circle
			(at 0 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "18" thru_hole circle
			(at 0 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "19" thru_hole circle
			(at 0 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "20" thru_hole circle
			(at 0 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x20_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 234.95 47.752 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 251.46 53.34 180)
		(descr "Through hole straight socket strip, 1x20, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x20 2.54mm single row")
		(property "Reference" "REF**"
			(at 0 2.77 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "PinSocket_1x20_P2.54mm_Vertical"
			(at 0 -51.03 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "21" thru_hole circle
			(at 0 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "22" thru_hole circle
			(at 0 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "23" thru_hole circle
			(at 0 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "24" thru_hole circle
			(at 0 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "25" thru_hole circle
			(at 0 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "26" thru_hole circle
			(at 0 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "27" thru_hole circle
			(at 0 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "28" thru_hole circle
			(at 0 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "29" thru_hole circle
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "30" thru_hole circle
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "31" thru_hole circle
			(at 0 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "32" thru_hole circle
			(at 0 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "33" thru_hole circle
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "34" thru_hole circle
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "35" thru_hole circle
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "36" thru_hole circle
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "37" thru_hole circle
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "C")
		)
		(pad "38" thru_hole circle
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "39" thru_hole circle
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "B")
		)
		(pad "40" thru_hole circle
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "A")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x20_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 228.854 41.91)
		(end 228.854 105.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.854 105.41)
		(end 234.95 105.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.95 105.41)
		(end 234.95 110.49)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.95 110.49)
		(end 252.73 110.49)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 105.41)
		(end 258.826 105.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 110.49)
		(end 252.73 105.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 258.826 41.91)
		(end 228.854 41.91)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 258.826 105.41)
		(end 258.826 41.91)
		(layer "Edge.Cuts")
	)
	(gr_text "3v3"
		(at 237.49 62.738 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 235.204 59.055 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "TEMP"
		(at 237.49 69.342 0)
		(layer "F.SilkS")
	)
	(gr_text "ANALOG X"
		(at 237.744 73.66 0)
		(layer "F.SilkS")
	)
	(gr_text "ANALOG Y"
		(at 237.744 77.724 0)
		(layer "F.SilkS")
	)
	(gr_text "ALT PEDAL"
		(at 237.744 81.788 0)
		(layer "F.SilkS")
	)
	(gr_text "CAM SCL"
		(at 237.744 86.995 0)
		(layer "F.SilkS")
	)
	(gr_text "CAM SDA"
		(at 237.744 89.662 0)
		(layer "F.SilkS")
	)
	(gr_text "RUMBLE"
		(at 237.744 100.584 0)
		(layer "F.SilkS")
	)
	(gr_text "SOLENOID"
		(at 237.744 102.87 0)
		(layer "F.SilkS")
	)
	(gr_text "OLED SDA"
		(at 252.984 86.995 0)
		(layer "F.SilkS")
	)
	(gr_text "OLED SCL"
		(at 252.984 89.535 0)
		(layer "F.SilkS")
	)
	(gr_text "NEOPIXEL"
		(at 252.984 91.948 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO2"
		(at 237.1852 92.0496 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO1"
		(at 237.2106 94.5642 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO10"
		(at 237.617 66.7766 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 237.744 53.975 0)
		(layer "F.SilkS")
	)
	(gr_text "Waveshare ESP32-S3-Pico / RP2040-Pico"
		(at 243.84 44.196 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 237.49 71.755 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 237.49 84.328 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 237.49 97.028 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 56.515 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 59.055 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 61.595 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 64.135 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 66.675 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 79.375 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 81.915 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 84.455 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 86.995 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 89.535 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "UP"
		(at 254.508 74.295 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 255.27 59.055 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 255.27 71.755 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 255.27 84.455 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 255.27 97.155 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "LEFT"
		(at 255.524 79.375 0)
		(layer "F.SilkS")
	)
	(gr_text "START"
		(at 256.032 64.135 0)
		(layer "F.SilkS")
	)
	(gr_text "HOME"
		(at 256.032 69.215 0)
		(layer "F.SilkS")
	)
	(gr_text "DOWN"
		(at 256.032 76.962 0)
		(layer "F.SilkS")
	)
	(gr_text "PUMP"
		(at 256.032 94.615 0)
		(layer "F.SilkS")
	)
	(gr_text "RIGHT"
		(at 256.286 81.915 0)
		(layer "F.SilkS")
	)
	(gr_text "PEDAL"
		(at 256.286 99.695 0)
		(layer "F.SilkS")
	)
	(gr_text "SELECT"
		(at 256.794 66.675 0)
		(layer "F.SilkS")
	)
	(gr_text "TRIGGER"
		(at 257.302 102.235 0)
		(layer "F.SilkS")
	)
	(gr_text "A BUTTON"
		(at 258.318 53.975 0)
		(layer "F.SilkS")
	)
	(gr_text "C BUTTON"
		(at 258.318 61.595 0)
		(layer "F.SilkS")
	)
	(gr_text "B BUTTON"
		(at 258.445 56.515 0)
		(layer "F.SilkS")
	)
	(gr_text "3v3"
		(at 241.3 62.865 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 252.349 49.022 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 236.474 62.738 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 247.269 56.515 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 59.055 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 61.595 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 64.135 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 66.675 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 79.375 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 81.915 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 84.455 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 86.995 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.269 89.535 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "UP"
		(at 254.635 74.295 0)
		(layer "B.SilkS")
	)
	(gr_text "LEFT"
		(at 255.651 79.375 0)
		(layer "B.SilkS")
	)
	(gr_text "START"
		(at 256.159 64.135 0)
		(layer "B.SilkS")
	)
	(gr_text "HOME"
		(at 256.159 69.215 0)
		(layer "B.SilkS")
	)
	(gr_text "DOWN"
		(at 256.159 76.962 0)
		(layer "B.SilkS")
	)
	(gr_text "PUMP"
		(at 256.159 94.615 0)
		(layer "B.SilkS")
	)
	(gr_text "RIGHT"
		(at 256.413 81.915 0)
		(layer "B.SilkS")
	)
	(gr_text "PEDAL"
		(at 256.54 99.695 0)
		(layer "B.SilkS")
	)
	(gr_text "SELECT"
		(at 256.921 66.675 0)
		(layer "B.SilkS")
	)
	(gr_text "TRIGGER"
		(at 257.429 102.235 0)
		(layer "B.SilkS")
	)
	(gr_text "A BUTTON"
		(at 258.064 53.975 0)
		(layer "B.SilkS")
	)
	(gr_text "B BUTTON"
		(at 258.064 56.515 0)
		(layer "B.SilkS")
	)
	(gr_text "C BUTTON"
		(at 258.064 61.595 0)
		(layer "B.SilkS")
	)
	(gr_text "Waveshare ESP32-S3-Pico / RP2040-Pico"
		(at 243.84 44.196 0)
		(layer "B.SilkS")
	)
	(gr_text "TEMP"
		(at 237.363 69.342 0)
		(layer "B.SilkS")
	)
	(gr_text "ANALOG X"
		(at 237.617 73.66 0)
		(layer "B.SilkS")
	)
	(gr_text "ANALOG Y"
		(at 237.617 77.724 0)
		(layer "B.SilkS")
	)
	(gr_text "ALT PEDAL"
		(at 237.617 81.915 0)
		(layer "B.SilkS")
	)
	(gr_text "CAM SCL"
		(at 237.617 87.0204 0)
		(layer "B.SilkS")
	)
	(gr_text "CAM SDA"
		(at 237.617 89.662 0)
		(layer "B.SilkS")
	)
	(gr_text "RUMBLE"
		(at 237.617 100.584 0)
		(layer "B.SilkS")
	)
	(gr_text "SOLENOID"
		(at 237.617 102.87 0)
		(layer "B.SilkS")
	)
	(gr_text "OLED SDA"
		(at 252.857 86.995 0)
		(layer "B.SilkS")
	)
	(gr_text "OLED SCL"
		(at 252.857 89.535 0)
		(layer "B.SilkS")
	)
	(gr_text "NEOPIXEL"
		(at 252.857 91.948 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO2"
		(at 237.3122 92.0242 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO1"
		(at 237.4392 94.5896 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO10"
		(at 237.7694 66.675 0)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 237.871 53.975 0)
		(layer "B.SilkS")
	)
	(gr_text "3v3"
		(at 241.3 62.865 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 255.651 49.022 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "B"
		(at 243.84 73.152 0)
		(layer "B.SilkS")
	)
	(gr_text "A"
		(at 243.84 95.758 0)
		(layer "B.SilkS")
	)
	(gr_text "C"
		(at 243.967 50.165 0)
		(layer "B.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(name "GND")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 228.854 41.91) (xy 258.826 41.91) (xy 258.826 104.14) (xy 228.854 104.14)
			)
		)
	)
	(zone
		(net 1)
		(net_name "VCC")
		(layers "F.Cu" "B.Cu")
		(name "VCC")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 232.41 59.69) (xy 240.03 59.69) (xy 240.03 64.77) (xy 232.41 64.77)
			)
		)
	)
	(embedded_fonts no)
)
