(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(comment 4 "AISLER Project ID: UDKLLJUE")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "VCC")
	(net 2 "GND")
	(net 3 "A")
	(net 4 "B")
	(net 5 "C")
	(footprint ""
		(layer "F.Cu")
		(at 243.84 63.5)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "Library:pad_2Dmm_1Fmm"
		(layer "F.Cu")
		(at 254 60.96)
		(property "Reference" "REF**"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "pad_2Dmm_1Fmm"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 81.28)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 71.12)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 91.44)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 63.5)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 99.06)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 83.82)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 241.3 81.28)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 53.34)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 76.2)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 53.34)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 83.82)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 86.36)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 73.66)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 66.04)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 246.38 58.42)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 58.42)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 101.6)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 86.367588)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 243.84 106.68)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 88.9)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 50.8)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 93.98)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "F.Cu")
		(at 241.59 75.08 90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "REF**"
			(at 3.25 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_PUSH_6mm"
			(at 3.75 6.7 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "B"
			(at 3.25 2.25 0)
			(unlocked yes)
			(layer "F.Cu")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "B")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "B")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 241.3 58.42)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "F.Cu")
		(at 241.59 97.94 90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "REF**"
			(at 3.25 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_PUSH_6mm"
			(at 3.75 6.7 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "A"
			(at 3.25 2.25 0)
			(unlocked yes)
			(layer "F.Cu")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "A")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "A")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 55.88)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 81.28)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 78.74)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 99.06)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "F.Cu")
		(at 241.59 52.22 90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "REF**"
			(at 3.25 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_PUSH_6mm"
			(at 3.75 6.7 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "C"
			(at 3.25 2.25 0)
			(unlocked yes)
			(layer "F.Cu")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "C")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "C")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 236.22 101.6)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 241.3 63.5)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 78.74)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 246.38 81.28)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 93.98)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 246.38 63.5)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 246.38 86.36)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 88.9)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 60.96)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 241.3 86.36)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 71.12)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 250.5964 98.7552)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 243.84 81.28)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 68.58)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 254 55.88)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 58.42)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 86.36)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 91.44)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 233.68 66.04)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x22_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 256.54 48.26 180)
		(descr "Through hole straight socket strip, 1x22, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x22 2.54mm single row")
		(property "Reference" "REF**"
			(at 0 2.77 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "PinSocket_1x22_P2.54mm_Vertical"
			(at 0 -56.11 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "23" thru_hole circle
			(at 0 -53.34 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "24" thru_hole circle
			(at 0 -50.8 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "25" thru_hole circle
			(at 0 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "26" thru_hole circle
			(at 0 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "27" thru_hole circle
			(at 0 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "28" thru_hole circle
			(at 0 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "29" thru_hole circle
			(at 0 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "30" thru_hole circle
			(at 0 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "31" thru_hole circle
			(at 0 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "32" thru_hole circle
			(at 0 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "33" thru_hole circle
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "B")
		)
		(pad "34" thru_hole circle
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "A")
		)
		(pad "35" thru_hole circle
			(at 0 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "36" thru_hole circle
			(at 0 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "37" thru_hole circle
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "38" thru_hole circle
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "39" thru_hole circle
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "40" thru_hole circle
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "C")
		)
		(pad "41" thru_hole circle
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "42" thru_hole circle
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "43" thru_hole circle
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "44" thru_hole circle
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x22_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x22_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 231.14 48.26 180)
		(descr "Through hole straight socket strip, 1x22, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x22 2.54mm single row")
		(property "Reference" "REF**"
			(at 0 2.77 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "PinSocket_1x22_P2.54mm_Vertical"
			(at 0 -56.11 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "3" thru_hole circle
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "5" thru_hole circle
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "6" thru_hole circle
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "7" thru_hole circle
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "8" thru_hole circle
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "9" thru_hole circle
			(at 0 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "10" thru_hole circle
			(at 0 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "11" thru_hole circle
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "12" thru_hole circle
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole circle
			(at 0 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "14" thru_hole circle
			(at 0 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole circle
			(at 0 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "16" thru_hole circle
			(at 0 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "17" thru_hole circle
			(at 0 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "18" thru_hole circle
			(at 0 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "19" thru_hole circle
			(at 0 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "20" thru_hole circle
			(at 0 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "21" thru_hole circle
			(at 0 -50.8 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(pad "22" thru_hole circle
			(at 0 -53.34 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x22_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 250.825 98.806 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(gr_line
		(start 228.854 41.91)
		(end 228.854 105.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.854 105.41)
		(end 234.95 105.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.95 105.41)
		(end 234.95 110.49)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.95 110.49)
		(end 252.73 110.49)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 105.41)
		(end 258.826 105.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 110.49)
		(end 252.73 105.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 258.826 41.91)
		(end 228.854 41.91)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 258.826 105.41)
		(end 258.826 41.91)
		(layer "Edge.Cuts")
	)
	(gr_text "3v3"
		(at 234.95 100.838 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 233.299 48.895 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "NEOPIXEL"
		(at 235.077 53.975 0)
		(layer "F.SilkS")
	)
	(gr_text "CAM SCL"
		(at 235.077 66.6496 0)
		(layer "F.SilkS")
	)
	(gr_text "ALT PEDAL"
		(at 235.077 69.088 0)
		(layer "F.SilkS")
	)
	(gr_text "CAM SDA"
		(at 235.077 74.295 0)
		(layer "F.SilkS")
	)
	(gr_text "OLED SDA"
		(at 235.077 76.835 0)
		(layer "F.SilkS")
	)
	(gr_text "SOLENOID"
		(at 235.077 79.375 0)
		(layer "F.SilkS")
	)
	(gr_text "RUMBLE"
		(at 235.077 81.915 0)
		(layer "F.SilkS")
	)
	(gr_text "OLED SCL"
		(at 235.077 84.455 0)
		(layer "F.SilkS")
	)
	(gr_text "TEMP SENSOR"
		(at 235.077 89.535 0)
		(layer "F.SilkS")
	)
	(gr_text "ANALOG Y"
		(at 235.077 92.075 0)
		(layer "F.SilkS")
	)
	(gr_text "ANALOG X"
		(at 235.077 94.615 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO13"
		(at 235.077 56.4896 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO11"
		(at 235.077 61.5188 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO10"
		(at 235.077 64.0588 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO3"
		(at 235.077 71.755 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO12"
		(at 235.1024 58.9534 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO7"
		(at 235.1024 86.9442 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 235.1786 51.4858 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO19"
		(at 248.539 53.8734 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO20"
		(at 248.6152 56.515 0)
		(layer "F.SilkS")
	)
	(gr_text "YD-ESP32-S3 WROOM1-DevKitC-1-N16R8"
		(at 243.84 44.196 0)
		(layer "F.SilkS")
	)
	(gr_text "PEDAL"
		(at 252.476 61.595 0)
		(layer "F.SilkS")
	)
	(gr_text "PUMP"
		(at 252.603 66.675 0)
		(layer "F.SilkS")
	)
	(gr_text "HOME"
		(at 252.603 71.755 0)
		(layer "F.SilkS")
	)
	(gr_text "SELECT"
		(at 252.603 79.375 0)
		(layer "F.SilkS")
	)
	(gr_text "START"
		(at 252.603 81.915 0)
		(layer "F.SilkS")
	)
	(gr_text "UP"
		(at 252.603 84.455 0)
		(layer "F.SilkS")
	)
	(gr_text "DOWN"
		(at 252.603 86.995 0)
		(layer "F.SilkS")
	)
	(gr_text "LEFT"
		(at 252.603 89.535 0)
		(layer "F.SilkS")
	)
	(gr_text "RIGHT"
		(at 252.603 92.075 0)
		(layer "F.SilkS")
	)
	(gr_text "TRIGGER"
		(at 252.603 94.615 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 254.508 48.895 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 254.508 51.435 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "C BUTTON"
		(at 254.508 59.055 0)
		(layer "F.SilkS")
	)
	(gr_text "A BUTTON"
		(at 254.508 74.295 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 254.508 102.235 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "B BUTTON"
		(at 254.635 76.835 0)
		(layer "F.SilkS")
	)
	(gr_text "3v3"
		(at 238.506 101.346 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 243.7892 85.1154 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 243.8146 62.1792 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 243.84 102.87 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 233.934 100.838 0)
		(layer "B.SilkS")
	)
	(gr_text "PEDAL"
		(at 252.73 61.595 0)
		(layer "B.SilkS")
	)
	(gr_text "PUMP"
		(at 252.73 66.675 0)
		(layer "B.SilkS")
	)
	(gr_text "HOME"
		(at 252.73 71.755 0)
		(layer "B.SilkS")
	)
	(gr_text "SELECT"
		(at 252.73 79.375 0)
		(layer "B.SilkS")
	)
	(gr_text "START"
		(at 252.73 81.915 0)
		(layer "B.SilkS")
	)
	(gr_text "UP"
		(at 252.73 84.455 0)
		(layer "B.SilkS")
	)
	(gr_text "DOWN"
		(at 252.73 86.995 0)
		(layer "B.SilkS")
	)
	(gr_text "LEFT"
		(at 252.73 89.535 0)
		(layer "B.SilkS")
	)
	(gr_text "RIGHT"
		(at 252.73 92.075 0)
		(layer "B.SilkS")
	)
	(gr_text "TRIGGER"
		(at 252.73 94.615 0)
		(layer "B.SilkS")
	)
	(gr_text "C BUTTON"
		(at 254.254 59.055 0)
		(layer "B.SilkS")
	)
	(gr_text "A BUTTON"
		(at 254.254 74.295 0)
		(layer "B.SilkS")
	)
	(gr_text "B BUTTON"
		(at 254.254 76.835 0)
		(layer "B.SilkS")
	)
	(gr_text "YD-ESP32-S3 WROOM1-DevKitC-1-N16R8"
		(at 243.84 44.196 0)
		(layer "B.SilkS")
	)
	(gr_text "NEOPIXEL"
		(at 234.95 53.975 0)
		(layer "B.SilkS")
	)
	(gr_text "CAM SCL"
		(at 234.95 66.675 0)
		(layer "B.SilkS")
	)
	(gr_text "ALT PEDAL"
		(at 234.95 69.215 0)
		(layer "B.SilkS")
	)
	(gr_text "CAM SDA"
		(at 234.95 74.295 0)
		(layer "B.SilkS")
	)
	(gr_text "OLED SDA"
		(at 234.95 76.835 0)
		(layer "B.SilkS")
	)
	(gr_text "SOLENOID"
		(at 234.95 79.375 0)
		(layer "B.SilkS")
	)
	(gr_text "RUMBLE"
		(at 234.95 81.915 0)
		(layer "B.SilkS")
	)
	(gr_text "OLED SCL"
		(at 234.95 84.455 0)
		(layer "B.SilkS")
	)
	(gr_text "TEMP SENSOR"
		(at 234.95 89.535 0)
		(layer "B.SilkS")
	)
	(gr_text "ANALOG Y"
		(at 234.95 92.075 0)
		(layer "B.SilkS")
	)
	(gr_text "ANALOG X"
		(at 234.95 94.615 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO11"
		(at 235.077 61.468 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO13"
		(at 235.204 56.515 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO12"
		(at 235.204 59.055 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO3"
		(at 235.204 71.755 0)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 235.3056 51.4096 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO10"
		(at 235.331 64.135 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO7"
		(at 235.331 86.995 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO19"
		(at 248.666 53.975 0)
		(layer "B.SilkS")
	)
	(gr_text "GPIO20"
		(at 248.666 56.515 0)
		(layer "B.SilkS")
	)
	(gr_text "3v3"
		(at 238.506 101.346 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 243.84 62.23 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 243.84 85.09 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 247.142 102.87 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "B"
		(at 243.84 73.152 0)
		(layer "B.SilkS")
	)
	(gr_text "A"
		(at 243.84 95.758 0)
		(layer "B.SilkS")
	)
	(gr_text "C"
		(at 243.967 50.165 0)
		(layer "B.SilkS")
	)
	(gr_text_box "USB OTG"
		(start 232.41 44.7675)
		(end 240.03 46.6725)
		(margins 1.0025 1.0025 1.0025 1.0025)
		(layer "F.SilkS")
		(border yes)
	)
	(gr_text_box "USB UART"
		(start 247.65 44.7675)
		(end 255.27 46.6725)
		(margins 1.0025 1.0025 1.0025 1.0025)
		(layer "F.SilkS")
		(border yes)
	)
	(gr_text_box "USB\nOTG"
		(start 234.061 45.593)
		(end 239.649 50.165)
		(margins 1.0025 1.0025 1.0025 1.0025)
		(layer "B.SilkS")
		(border yes)
	)
	(gr_text_box "USB\nUART"
		(start 248.031 45.593)
		(end 253.619 50.165)
		(margins 1.0025 1.0025 1.0025 1.0025)
		(layer "B.SilkS")
		(border yes)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(name "GND")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 228.854 41.91) (xy 258.826 41.91) (xy 258.826 104.14) (xy 228.854 104.14)
			)
		)
	)
	(zone
		(net 1)
		(net_name "VCC")
		(layers "F.Cu" "B.Cu")
		(name "VCC")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 229.893986 97.79) (xy 237.513986 97.79) (xy 237.513986 102.87) (xy 229.893986 102.87)
			)
		)
	)
	(embedded_fonts no)
)
